{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":22,"rows_kept":26,"merged":[[1,0,1,21],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,8],[2,9,2,10],[2,11,2,20],[2,21,4,21],[3,7,4,7],[3,8,4,8],[3,9,4,9],[3,10,4,10],[3,11,3,12],[3,13,3,14],[3,15,3,16],[3,17,3,18],[3,19,3,20],[25,0,25,21]],"flags":["formulas_cached_only"]}
["附表："]
["常州市农村河道(包括通航河道)坍塌情况调查表"]
["市、区名称","乡镇名称","河道名称","河道级别","河道长度（千米）","详细起止点","流经圩区名称","坍塌长度  (千米)",null,"现有驳岸长度(千米)",null,"沿河水利建筑物(座)",{"$nulls":9},"备注"]
[{"$nulls":7},"一般坍塌","严重坍塌","2005年前","2005年后","泵站",null,"闸         (含圩口闸)",null,"涵洞",null,"桥梁",null,"其它"]
[{"$nulls":11},"总数","影响数量","总数","影响数量","总数","影响数量","总数","影响数量","总数","影响数量"]
{"$rows_empty":20}
["注：坍塌长度和现有驳岸长度应填河道两岸情况的累加数。沿河水利建筑物中影响数量指河岸、河坡坍塌影响建筑物安全的数量。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}